## The smart solution

# Motorised A-opener 2.1 – versatile, secure, convenient

More flexibility, more security, more comfort – the new A-opener 2.1 from KFV for the AS 3500 and AS 3600 automatic multi-point locks provides tangible benefits for fabricators and end users. With its help, the automatic multi-point locking systems can be upgraded to an electromechanical version. The size range of the A-opener has been extended significantly in the new 2.1 version. The combination with separable power supplies such as tappet contacts is now possible. This gives the door a discreet, appealing appearance and makes connection and installation extremely easy. Room comfort goes hand in hand with easy fabrication. The A-opener 2.1 is suitable for house and apartment entrance doors of all frame materials.

#### Versatile comfort functions

The implementation of digital communication via the SI-BUS is a really unique feature. With the help of this, fabricators can now also use the optional SI-BUS converter and the SI-BUS analytical tool. The latter is available for free downloading on the SIEGENIA website. For the sales negotiation, this means that fabricators score highly here as they can provide their customers with considerably more security and comfort features than have hitherto been available. The option for combination with a wide range of access control systems - from KFVkeyless to the fingerprint scanner, up to radio remote control and transponder systems - provides a high degree of flexibility. Even the connection to smart home systems is possible thanks to the WLAN-capable smart module universal and control via somfy io-homecontrol®. This brings significant gains in terms of comfort and security and provides maximum flexibility due to subsequent updates and system extensions.

Another clear advantage is the optimised motor, which is considerably faster and quieter than previously. This creates a high degree of ease of use for end users. Fabricators also benefit in production from the strengths of the motor based on the tried and tested version for KFV GENIUS. For the functional test of the multi-point lock in the factory, you now receive information on the current operating status via the LED status indicator. Moreover, you can conveniently adapt the volume of the buzzer via a button.

#### AS 3600: Security with additional benefits

For example, combined with the AS 3600 automatic multi-point lock from KFV, the new A-opener 2.1 offers end users permanent security and high convenience in the locking and unlocking of house entrance doors. The principle of the efficient duo is as simple as it is effective: As soon as both automatic falling bolts of the auxiliary boxes are activated by the mechanical trigger, they initiate closing and disengage at 20 mm. At the same time, the two hook bolts of AS 3600 grip into the frame parts. This ensures fourfold security and burglar resistance up to RC2 without forcing end users to actively think about locking the door. A positive side effect: The door is reliably protected by the elements against warping and thus offers permanent room comfort. The locking elements can be easily retracted with the lever handle or the key. This makes the opening process incredibly easy and convenient.

#### Caption

Image database: SIEGENIA

*Image: SIE\_KFV\_A-opener 2.1\_detail.jpg*

More flexibility, more security, more comfort – with a significantly extended size range, the new A-opener 2.1 provides tangible benefits for fabricators and end users.

|  |  |  |
| --- | --- | --- |
| Publisher  SIEGENIA GROUP  Marketing Communications  Industriestraße 1-3  D-57234 Wilnsdorf Germany  Phone: +49 271 3931-412  Fax: +49 271 3931-77412  E-mail: pr@siegenia.com  www.siegenia.com/en | Edited by / Contact  Kemper Kommunikation  Kirsten Kemper  Feuerwehrstr. 42  D-51588 Nuembrecht Germany Phone: +49 2293 909890  Fax: +49 2293 909891  E-mail: info@kemper-kommunikation.de  www.kemper-kommunikation.de | Text details  Pages: 2  Words: 506  Characters: 3,177 (including spaces)  Created: 2018-03-21 |
| Please send us a sample copy of any publication containing this text or these images. | | |